Sequence probe: 3 frames x 2 group(s) on COM5 at 38400 8N1
FRAME 1: 00 00 00 00 80 DA
FRAME 2: 00 00 40 60 30 4A
FRAME 3: 00 00 00 00 80 DA
BASELINE heartbeat-compatible RX: 6 bytes, offset 0, 1 frames + 0 bytes
BEGIN group 1/2
21:17:06.565  TX group=1 frame=1 len=006  00 00 00 00 80 DA
21:17:06.565  RX group=1 frame=1 heartbeat-compatible RX: 6 bytes, offset 0, 1 frames + 0 bytes
21:17:07.072  TX group=1 frame=2 len=006  00 00 40 60 30 4A
21:17:07.072  RX group=1 frame=2 ANOMALY 18 RX bytes; first mismatch at byte 6: got 07, heartbeat offset 0 expected 00
21:17:07.072  RX group=1 frame=2 raw 00 00 00 00 80 DA 07 80 50 58 26 F3 07 80 50 58 26 F3
21:17:07.580  TX group=1 frame=3 len=006  00 00 00 00 80 DA
21:17:07.580  RX group=1 frame=3 ANOMALY 18 RX bytes; first mismatch at byte 0: got 07, heartbeat offset 0 expected 00
21:17:07.580  RX group=1 frame=3 raw 07 80 50 58 26 F3 00 00 00 00 80 DA 00 00 00 00 80 DA
GROUP 1 TAIL heartbeat-compatible RX: 18 bytes, offset 0, 3 frames + 0 bytes
BEGIN group 2/2
21:17:08.739  TX group=2 frame=1 len=006  00 00 00 00 80 DA
21:17:08.739  RX group=2 frame=1 heartbeat-compatible RX: 12 bytes, offset 0, 2 frames + 0 bytes
21:17:09.275  TX group=2 frame=2 len=006  00 00 40 60 30 4A
21:17:09.275  RX group=2 frame=2 heartbeat-compatible RX: 18 bytes, offset 0, 3 frames + 0 bytes
21:17:09.781  TX group=2 frame=3 len=006  00 00 00 00 80 DA
21:17:09.781  RX group=2 frame=3 heartbeat-compatible RX: 12 bytes, offset 0, 2 frames + 0 bytes
GROUP 2 TAIL heartbeat-compatible RX: 18 bytes, offset 0, 3 frames + 0 bytes
Anomalies: 2
